String WigaTopTemp "Temperatur [%s C]" {mqtt="<[mqm:/WigaTop/temp:state:default]"}
Number WigaTopTempNumber "Temperature [%.1f C]"
String WigaTopHum "Humidity [%s ]" {mqtt="<[mqm:/WigaTop/humidity:state:default]"}
String WigaTopStatus "Status [%s ]" {mqtt="<[mqm:/WigaTop/status:state:default]"}
Switch WigaR1 "Nr1" {mqtt=">[mqm:/WigaTop/relais/r1:command:ON:on], >[mqm:/WigaTop/relais/r1:command:OFF:off]"}
Switch WigaR2 "Nr2" {mqtt=">[mqm:/WigaTop/relais/r2:command:ON:on], >[mqm:/WigaTop/relais/r2:command:OFF:off]"}
Switch WigaR3 "Nr3" {mqtt=">[mqm:/WigaTop/relais/r3:command:ON:on], >[mqm:/WigaTop/relais/r3:command:OFF:off]"}
Switch WigaR4 "Nr4" {mqtt=">[mqm:/WigaTop/relais/r4:command:ON:on], >[mqm:/WigaTop/relais/r4:command:OFF:off]"}
String KellerTemp "Temperatur [%s C]" {mqtt="<[mqm:/keller/temp:state:default]"}
String KellerHum "Humidity [%s C]" {mqtt="<[mqm:/keller/humidity:state:default]"}
String KellerMotor "Drehzahl" {mqtt=">[mqm:/keller/drehz:command:*:default], <[mqm:/keller/upm:state:*:default]"}
Switch KellerMotorFrei "frei"  {mqtt=">[mqm:/keller/frei:command:ON:on], >[mqm:/keller/frei:command:OFF:off], <[mqm:/keller/state:state:state:default]"}
Switch KellerMotorleft "links"  {mqtt=">[mqm:/keller/left:command:ON:on], >[mqm:/keller/left:command:OFF:off]"}
Number TeichWasser "Wasserstand [%s cm]" {mqtt="<[mqm:/teich/wasser:state:default]"}
Switch TeichR1 "Zufluss" {mqtt=">[mqm:/teich/r1:command:ON:on], >[mqm:/teich/r1:command:OFF:of]"}
Switch TeichR2 "Steckdose" {mqtt=">[mqm:/teich/r2:command:ON:on], >[mqm:/teich/r2:command:OFF:of]"}
Number    Day_Period                        "Chart Period"
Number TeichStatus "Status [%s]" {mqtt="<[mqm:/teich/relais:state:default]"}
